# DigiBadge
An open source digital color communications badge
For information on what a "Color Communications Badge" is, see http://bitly.com/1jY0tzO

The "Regular" version of the DigiBadge runs off of an ATMega 168 microcontroller, and the "Hacker" version of the DigiBadge runs off of an ATMega 328 microcontroller like what you would find in an Arduino Uno.

To program one of the devices, select the "Arduino Pro or Pro Mini"
For the Hacker Badge, select the 3.3v 8MHz ATMega 328 processor
For the Regular Badge, select the 3.3v 8MHz ATMega 168 processor
