# configuration file generated by Bochs
plugin_ctrl: unmapped=1, biosdev=1, speaker=1, extfpuirq=1, parallel=1, serial=1
config_interface: textconfig
display_library: sdl
memory: host=256, guest=256
romimage: file="/usr/local/share/bochs/BIOS-bochs-latest", address=0x00000000, options=none
vgaromimage: file="/usr/local/share/bochs/VGABIOS-lgpl-latest"
boot: cdrom
floppy_bootsig_check: disabled=0
# no floppya
# no floppyb
ata0: enabled=1, ioaddr1=0x000001f0, ioaddr2=0x000003f0, irq=14
ata0-master: type=cdrom, path="/dev/cdrom0", status=inserted, model="Generic 1234", biosdetect=auto
ata0-slave: type=none
ata1: enabled=1, ioaddr1=0x00000170, ioaddr2=0x00000370, irq=15
ata1-master: type=none
ata1-slave: type=none
ata2: enabled=0
ata3: enabled=0
optromimage1: file=none
optromimage2: file=none
optromimage3: file=none
optromimage4: file=none
optramimage1: file=none
optramimage2: file=none
optramimage3: file=none
optramimage4: file=none
pci: enabled=1, chipset=i440fx, slot1=pcivga
vga: extension=vbe, update_freq=5, realtime=1
cpu: count=1, ips=4000000, model=bx_generic, reset_on_triple_fault=1, cpuid_limit_winnt=0, ignore_bad_msrs=1, mwait_is_nop=0
cpuid: level=6, stepping=3, model=3, family=6, vendor_string="GenuineIntel", brand_string="              Intel(R) Pentium(R) 4 CPU        "
cpuid: mmx=1, apic=xapic, simd=sse2, sse4a=0, misaligned_sse=0, sep=1, movbe=0, adx=0
cpuid: aes=0, sha=0, xsave=0, xsaveopt=0, smep=0, smap=0, mwait=1
print_timestamps: enabled=0
port_e9_hack: enabled=0
private_colormap: enabled=0
clock: sync=realtime, time0=local, rtc_sync=1
# no cmosimage
# no loader
log: -
logprefix: %t%e%d
debug: action=ignore
info: action=report
error: action=report
panic: action=fatal
keyboard: type=mf, serial_delay=250, paste_delay=100000, user_shortcut=none
mouse: type=ps2, enabled=0, toggle=ctrl+mbutton
speaker: enabled=1, mode=gui
parport1: enabled=1, file=none
parport2: enabled=0
com1: enabled=1, mode=null
com2: enabled=0
com3: enabled=0
com4: enabled=0
